Information

NOTIFICATION

ICQ Pager.
If you’re Victim has a Dynamic ip Address it is good to have some Kind of notification, so once there ip address changes you will get there new ip. Oh and victim doesn't need to have ICQ installed to send the pager to your ICQ number.

CGI Logger
This is good as an alternative to an ICQ pager, if you don’t know what CGI logger is then go to http://www.black-fire.net for more info on what a CGI Logger is and what is dues.

General Settings

Make LAN Visible

If checked, this option will leave the server visible-- this is mainly used for testing. If the server is visible it will not install or put itself in the registry, so that means if you close the server it will not restart on windows boot. But, if the server is hidden then it will install and put itself into the registry, so it will start up on windows Boot.

IP Settings
You will need to put your ip in here for the Server to connect to. If you want to know what your ip is just click the “!” , and it will popup in the Text Box.

The reason why you need to put the ip in the Text Box.
If the server detects that the victim you are trying to use LANfiltrator on is on a LAN then it will connect to your ip, the ip that you put in the Text box. It only does this because you can’t connect directly to a computer that is on a LAN or a Proxy with the client, but a computer that is on a LAN or Proxy can connect to you, as long as you are on a direct connection and not a LAN yourself. So keep this option checked unless you know for a fact that the victim is directly connected to the internet. If they are not on a LAN and you have this option checked, it will just ignore it and open the server socket, and listen for your connection with the client like a normal Trojan.

Dynamic ip.
1st of all what is a Dynamic ip.
A dynamic IP is an IP that is received from a DHCP server (internet server) which is given each time it is connected to the internet.  This IP will often be different every time you connect to the internet. .

Ok, so if you are on a modem be confident that you have a dynamic ip. Even some cable connections might have a dynamic ip.
All you need to do is upload a text document with your ip in it to a website, and the server will automatically download from, and start to connect to the ip that is in the file. So essentially, when you log on the net upload the text document and the server will download the document once they are on the net. To get a sample file ready for upload just click the ‘!’ to get a text document file ready for upload, once generat12:35 AM 3/07/200112:35 AM 3/07/2001ed you can rename the document to what ever you like and then upload it to the internet and put the link to the site in the edit box.
